   *******************************************************************************
   *******************************************************************************
   ***                                                                         ***
   ***                                                                         ***
   ***    ***   ***    ***     ******   *********       *          ********    ***
   ***    ***   ****   ***    *******   *********      ***         **    **    ***
   ***    ***   *****  ***   ****          ***        *****        **    **    ***
   ***    ***   ****** ***    ****         ***       **   **       ********    ***
   ***    ***   *** ******     *****       ***      *********      *****       ***
   ***    ***   ***  *****        ***      ***     ***********     *******     ***
   ***    ***   ***   ****   ********      ***    ***       ***    ***  ***    ***
   ***    ***   ***    ***   *******       ***   ***         ***   ***    **   ***
   ***                                                                         ***
   ***                                                                         ***
   *******************************************************************************
   *******************************************************************************


   VERY VERY IMPORTANT!!!
   - REBOOT THE CAMERA ONCE BEFORE THE UPDATE!!! In the Web interface go to: Software - Restart
     Only after you have restarted the camera, please to the update.
   - Never disconnect the power supply during the update
   - The update can take up to 12 minutes since the camera will automatically put all
     settings back after updating so that you dont loose any settings
   - If there are disconnections in your network, INSTAR accepts no
     Warranty claims caused by a faulty update process
   - Always wait until the countdown has finished. In some cases it can be that the
     camera needs more time then the countdown... so please wait until your camera
     is reachable again.



   How to install the new firmware?
   - Open the web interface of your camera
   - On the left side please click on "Software - Update"
   - Please choose by "Select" the file update.pkg
   - Press "submit" and the update will be sent to the camera
   - After about 300 secounds the update process will be finished
   - In some cases please make sure you clear the cache of your webbrowser in order 
     to see the new features




   What is new in version 1.22 (756) ?

   - General bugfixes and layout changes




   What is new in version 1.21 (752) ?

   - Alarm recordings up to 45 seconds
   - Touch support for drawing alarm areas
   - IP addresses can be logged in the syslog. Activate under user settings!
   - The alarm area will be specified in the log when using linked alarm
   - PUSH test button added. Push must be activated and QR code must be scanned prior to using the test button
   - WiFi and network settings can now be exempted from the factory reset
   - An alarm event can be trigger by the following CGI command - /param.cgi?cmd=pushhostalarm
   - When using DHCP, camera will claim an unique DHCP hostname
   - Built-in recovery functionalities to restore cameras with a failed update. Downgrades will be limited to this exact version.
   - General bugfixes and layout changes




   What is new in version 1.20 (740) ?

   - Simple 1-Click update method
   - Offline update with traditional PKG file is optionally available
   - Alarm areas can be activated at preconfigured times
   - General bugfixes and layout changes




   What is new in version 1.19 (653) ?

   - Problem solved with P2P
   - General bugfixes and layout changes




   What is new in version 1.17 (643) ?

   - Fixed problem during automatic summer / winter changeover
   - Fixed problem with which the alarm sound could not be deactivated for IN-6014HD
   - New validation integrated for input fields
   - Security gap closed
   - General bugfixes and layout changes




   What is new in version 1.16 (620) ?

   - Problem solved when activating the cloud upload that after opening the settings again it does not show activated anymore.




   What is new in version 1.15 (617) ?

   - Problem fixed with P2P connection
   - Enhancements for the P2P connection speed
   - General bugfixes and layout changes




   What is new in version 1.14 (601) ?

   - user defined NTP time server is now possible
   - Problem solved with FTP upload
   - Problem solved with authentification when using MJPEG stream or snap.jpg
   - Problem solved that the camera will not restart after changing a port
   - Special character problem solved for Wifi, DDNS, FTP and Cloud passwords
   - Language Strings have been adjusted
   - General bugfixes and layout changes




   What is new in version 1.13 (586) ?

   - The INSTAR Cloud Recording platform is now available, for more information see: 
     https://cloud.instar.de
   - LAN and Wifi Mac address will now be both shown under "System - Info" (if your camera model has Wifi)
   - The preselection for GMX as the SMTP server was adjusted from mail.gmx.net to mail.gmx.de to prevent problems with the Telekom Speedport Router
   - General bugfixes and layout changes




   What is new in version 1.12 (555) ?

   - Alarm Server
   - Scheduled daily reboot
   - Email SMTP without authentication
   - Introducing new Wizard
   - User & Guest Accounts can be disabled
   - Syslog translations
   - Fixed issue with deleting camera name completely
   - H264 videos support for all ports in user and guest view
   - Fixed issue with certain email providers (e.g. GMX, web.de, Gmail, AOL)
   - Fixed issue where alarm input, audio alarm and motion detection did not work if activated at the same time
   - General bugfixes and layout changes

   For all Pan and Tilt cameras:
   - Cameras Park Position for PTZ models




   What is new in version 1.11 (431) ?

   - New h.264 video-stream using the RTMP protocol via the new RTMP Port (see Network > IP Configuration) which supports Flash Plugin
   - Two different MotionJPEG streams:
     1. MJPEG (Single-Image-Video directly from the camera - NEW and more robust)
     2. JPEG (Single-Image-Video directly from the Web Browser - works with every HTML Browser)
   - Privacy Mask - You can set up to 4 Areas that are completely 'blacked' out in the live video
   - Camera Settings are not deleted with an Update
   - H.264 Video Support for Linux via Flash (e.g. with Chromium)
   - Manual SD Card Recording via the Web Interface
   - Two different FTP folder modes:
     1. All Files in one directory
     2. Create a new folder every day
   - You can manually open (grey) and close (red) the alarm output relay using the web user interface (not available for IN-6001HD and IN-6014HD)
   - New and improved Software Updater (only available after this Update)
   - Camera connected to WiFi network can now switch to another WiFi network (a WiFi test is not possible due to technical reasons)

   For all Pan and Tilt cameras:
   - Tour Feature
   - One-Step Pan and Tilt control

   - General bugfixes and improvements




   What is new in version 1.10 (271) ?
  
   This update mainly includes bug fixes and code improvements

   - New (signed) version of the activeX control plugin
   - fixed issue with audio tone activation via multimedia > audio
   - fixed issue with cameras mobileresolution /tmpfs/auto.jpg used for MJPEG in lower resolution




   What is new in version 1.10 (264) ?

   This update mainly includes bug fixes and code improvements

   - fixed issue with photo series with fixed name (Bug from WebUI 1.9(213)
   - fixed issue with creating QR code
   - fixed issue with missing sub model number for updater
   - fixed issue with web browser caching the web sites (after the update and one first initial 
     reload of the webUI the code should completely be loaded from the camera)
   - fixed issue with showing wrong language afterReset, afterBackup and afterUpdate
   - fixed issue with video for linux machines
   - fixed issue with reloading webUI to new iframe level
   - fixed issue with loading the overlay with slow response time
   - general code improvement which should lead to singificant increase of the loading speed of 
     the webUI (especially via camera LAN IP)
   - general bugfixes, changes and typos




   What is new in version 1.9 ?
   - Push Notifications are now possible with our App InstarVision (iOS and Android)
   - ActiveX Plugin is now also supported for Chrome and Firefox on Windows
   - Scheduled activation and deactivation of the cameras IR LEDs
   - Solving issues with the 1und1 Email Server
   - A new integrated INSTAR Emailserver is now available to sent emails
   - A second Email receiver can now be added
   - PTZ limitations (for cameras with PTZ)
   - If an alarm is caused the camera can now move to a defined position (for cameras with PTZ)
   - Alarm signal can be played during alarm. The internal speaker or audio output will be used.
   - automatic wifi test
   - language detection through web browser
   - automatic status check of the SD card
   - New NTP Servers
   - Improvments, Bugfixes and TYPOS




   What is new in version 1.6 ?
   - Default SMTP settings for 1und1 adjusted
   - Problems with the audio function solved while using P2P
   - Small problem solved when saving alarm actions




   What is new in version 1.5 ?
   - Problems with the loss of Gateway is solved (this could have caused the camera 
     be not reachable anymore or that it doesnt sent any more alarm messages)
   - Extended SMTP settings, predefined standard SMTP servers
   - Refresh function when viewing the LOG file
   - Minor Bug fixes...




   What is new in version 1.4 ?
   - Video recording by schedule on SD card
   - Change the number of snapshots (email, FTP, SD) 
   - Resolution of snapshots 
   - Schedule for photo series 
   - Pre-selection of email providers 
   - Coupling of alarm input and motion detection (When an alarm triggers
     e.g. external motion, and the software of the camera also detects motion within 5
     seconds, then an alarm is generated) 
   - Problems with some email providers fixed (GMX, Web.de ...) 
   - Setup Wizard after reset the camera 
   - PTZ functions such as (deactivation of Justagefahrt, starting from position 1
     after restart, speeds etc ...)
   - Fixed GMT + 1 / daylight saving time issues 
   - Audio alarm (triggered by noise) 
   - Extension to the languages French and Chinese 
   - P2P Point to Point connection (supports external access regardless
     of the Internet connection via the App InstarVision). Thus, also
     connections over IPv6, mobile internet, etc. are possible. 
   - Minor bug fixes...